ERC report (2026-04-20T17:37:07-0400, Encoding UTF8)

***** Sheet /
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 36.83 mm): Symbol ESP32-WROOM1 Pin 15 [EN, Bidirectional, Line]
[power_pin_not_driven]: Input Power pin not driven by any Output Power pins
    ; error
    @(35.56 mm, 29.21 mm): Symbol #PWR05 Pin 1 [Power input, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 39.37 mm): Symbol ESP32-WROOM1 Pin 14 [VP, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 41.91 mm): Symbol ESP32-WROOM1 Pin 13 [VN, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 44.45 mm): Symbol ESP32-WROOM1 Pin 12 [D34, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 46.99 mm): Symbol ESP32-WROOM1 Pin 11 [D35, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 49.53 mm): Symbol ESP32-WROOM1 Pin 10 [D33, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 52.07 mm): Symbol ESP32-WROOM1 Pin 9 [D32, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 54.61 mm): Symbol ESP32-WROOM1 Pin 8 [D25, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 57.15 mm): Symbol ESP32-WROOM1 Pin 7 [D26, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 59.69 mm): Symbol ESP32-WROOM1 Pin 6 [D27, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 36.83 mm): Symbol ESP32-WROOM1 Pin 30 [D23, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 62.23 mm): Symbol ESP32-WROOM1 Pin 5 [D14, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 39.37 mm): Symbol ESP32-WROOM1 Pin 29 [D22, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 64.77 mm): Symbol ESP32-WROOM1 Pin 4 [D12, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 41.91 mm): Symbol ESP32-WROOM1 Pin 28 [TX0, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 44.45 mm): Symbol ESP32-WROOM1 Pin 27 [RX0, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(25.40 mm, 67.31 mm): Symbol ESP32-WROOM1 Pin 3 [D13, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 57.15 mm): Symbol ESP32-WROOM1 Pin 22 [D17, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 59.69 mm): Symbol ESP32-WROOM1 Pin 21 [D16, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 67.31 mm): Symbol ESP32-WROOM1 Pin 18 [D15, Bidirectional, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(55.88 mm, 69.85 mm): Symbol ESP32-WROOM1 Hidden pin 17 [GND, Bidirectional, Line]
[power_pin_not_driven]: Input Power pin not driven by any Output Power pins
    ; error
    @(97.79 mm, 29.21 mm): Symbol #PWR06 Pin 1 [Power input, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(52.07 mm, 158.75 mm): Symbol C8 Pin 1 [Passive, Line]
[pin_not_connected]: Pin not connected
    ; error
    @(52.07 mm, 166.37 mm): Symbol C8 Pin 2 [Passive, Line]
[footprint_link_issues]: The current configuration does not include the footprint library 'Library'.
    ; warning
    @(40.64 mm, 49.53 mm): Symbol ESP32-WROOM1 [ESP-WROOM-32]
[lib_symbol_issues]: The current configuration does not include the symbol library 'A1-KnockOffs'
    ; warning
    @(40.64 mm, 49.53 mm): Symbol ESP32-WROOM1 [ESP-WROOM-32]
[missing_unit]: Symbol SW1 has unplaced units [ B ]
    ; warning
    @(26.67 mm, 102.87 mm): Symbol SW1 [SW_DPDT_x2]
[lib_symbol_mismatch]: Symbol 'Conn_01x04_MountingPin' doesn't match copy in library 'Connector_Generic_MountingPin'
    ; warning
    @(113.03 mm, 49.53 mm): Symbol StepperConnection1 [Conn_01x04_MountingPin]

 ** ERC messages: 29  Errors 25  Warnings 4
