(footprint "ESP32-WROOM-SAVED"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2.4 GHz Wi-Fi and Bluetooth module https://docs.espressif.com/projects/esp-dev-kits/en/latest/esp32c3/esp32-c3-devkitm-1/index.html")
	(tags "esp32 esp32-c3 riscv risc-v wifi bluetooth ble")
	(property "Reference" "REF**"
		(at 12.7 38.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4e11e9b2-feae-41c4-8325-99667deef55a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ESP32-WROOM-SAVED"
		(at 12.7 40.64 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "25b8f628-13df-4e92-ac90-2836dc024f9b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "21122b41-f641-4c68-8180-0d1cc5cd0c77")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b4e7a260-42a4-4fe6-bced-d9b07281b709")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.27 -1.68)
		(end 26.67 -1.68)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1ca0204a-eae3-42f4-a97f-482a457850af")
	)
	(fp_line
		(start -1.27 37.24)
		(end -1.27 -1.68)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2bc775f9-a11f-4d07-af3a-8ddc7ece91fc")
	)
	(fp_line
		(start 26.67 -1.68)
		(end 24.13 37.24)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f20ad5f4-583a-4461-a6e7-d608c3cfe45a")
	)
	(fp_line
		(start 26.67 37.24)
		(end -1.27 37.24)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0671712f-4e5b-426b-9f8d-4aa9f4a7fa7f")
	)
	(fp_line
		(start -1.4 -7.35)
		(end -1.4 37.34)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d2f3a8bb-3c75-4100-97ca-edffeca9809a")
	)
	(fp_line
		(start -1.4 37.34)
		(end 26.8 37.34)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ab9973c2-48eb-4744-9e1f-1871c9805e66")
	)
	(fp_line
		(start 26.8 -7.35)
		(end -1.4 -7.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "de6ff2a0-a416-4bd0-af7f-19e3e7671869")
	)
	(fp_line
		(start 26.8 37.34)
		(end 26.8 -7.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4065d72a-a8a0-4c1e-b6ac-18ca9d635551")
	)
	(fp_line
		(start -1.27 -1.18)
		(end -1.27 37.235)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ba591c22-8281-48c3-b23f-1d3be93a2225")
	)
	(fp_line
		(start -1.27 -1.18)
		(end -0.83 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "084de9e7-2c3a-480f-a452-186a7f31b9df")
	)
	(fp_line
		(start -1.27 37.235)
		(end 26.67 37.235)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "31694135-2a21-4f0b-bb00-8d7bb12b6025")
	)
	(fp_line
		(start 4.83 -7.08)
		(end 18.03 -7.08)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "01ab237c-51ee-4aec-9ca4-d855789cd78d")
	)
	(fp_line
		(start 4.83 -1.675)
		(end -0.83 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "da407fff-d2ff-42d5-a646-e1b351224ae0")
	)
	(fp_line
		(start 4.83 -1.675)
		(end 4.83 -7.08)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "47176b27-908c-43ba-857b-bcd546f46320")
	)
	(fp_line
		(start 18.03 -7.08)
		(end 18.03 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f302fc52-5a6d-4bb8-a0c1-3b226a6664a8")
	)
	(fp_line
		(start 18.03 -1.675)
		(end 26.67 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9ce46ef0-7df6-4998-958d-fb7eaca17cdf")
	)
	(fp_line
		(start 26.67 37.235)
		(end 26.67 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "34c98e10-07fe-4179-a385-252d313b0314")
	)
	(fp_text user "Antenna"
		(at 12.7 -4.318 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "922f5726-92fb-45d9-ba7d-50b219dc9bad")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 12.7 17.78 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4d092454-ff91-41bb-8339-3fc32e967bc0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 31.435)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "bdcac96f-71d6-4938-83c4-5aafb9cc040e")
	)
	(pad "2" thru_hole circle
		(at 0 28.895)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "3c2be7da-89da-4ff6-9c0a-88fe9baef6f8")
	)
	(pad "3" thru_hole circle
		(at 0 26.355)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "e22c0a2d-a95b-4999-875b-549fac9470c8")
	)
	(pad "4" thru_hole circle
		(at 0 23.815)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "c1b2249e-1ce8-4ccb-8ce0-f758d92a07e4")
	)
	(pad "5" thru_hole circle
		(at 0 21.275)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "495d45fa-58a7-458e-ac66-b6a341bd53dc")
	)
	(pad "6" thru_hole circle
		(at 0 18.735)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "4b71babf-e40e-4726-aade-c3a51885cffb")
	)
	(pad "7" thru_hole circle
		(at 0 16.195)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "c07b00c0-b78d-4dcd-ba28-d7940b41cc74")
	)
	(pad "8" thru_hole circle
		(at 0 13.655)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "e088f660-9b35-41a9-862c-a4102b0f35f2")
	)
	(pad "9" thru_hole circle
		(at 0 11.115)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "fc268f5f-2ed9-4352-826a-9712dc845c38")
	)
	(pad "10" thru_hole circle
		(at 0 8.575)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "5ef4bd41-2e28-4b6f-a3c5-a193b72a0aa3")
	)
	(pad "11" thru_hole circle
		(at 0 6.035)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "bde8103a-273c-447d-bd71-99d46de61ec7")
	)
	(pad "12" thru_hole circle
		(at 0 3.495)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "8a13b0b6-cf46-4053-aaa2-210d999d4dd9")
	)
	(pad "13" thru_hole circle
		(at 0 0.955)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "d4fb13d1-509d-49fd-a143-86d4497ba294")
	)
	(pad "14" thru_hole circle
		(at 0 -1.585)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "39211a9a-0ec0-4713-80c1-ed626ad7d8e7")
	)
	(pad "15" thru_hole rect
		(at 0 -4.125)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "a83487a4-42d0-48be-b82b-1cd60cee081b")
	)
	(pad "16" thru_hole circle
		(at 25.4 31.435)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "06c7ee5b-4a55-4916-9723-3fe8427c41dc")
	)
	(pad "17" thru_hole circle
		(at 25.4 28.895)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "8f396d3a-40c2-4288-ae6d-20e97e705b22")
	)
	(pad "18" thru_hole circle
		(at 25.4 26.355)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "5e1da501-7df1-4df6-9ac9-bc1d2c3e9c62")
	)
	(pad "19" thru_hole circle
		(at 25.4 23.815)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "014e6c43-21fc-4283-971b-4ca3f4e492c9")
	)
	(pad "20" thru_hole circle
		(at 25.4 21.275)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "0e646a87-6dca-4412-bfe0-d92bc053f5e8")
	)
	(pad "21" thru_hole circle
		(at 25.4 18.735)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "6b8b2f8f-4e95-447c-843d-0e5458de18c5")
	)
	(pad "22" thru_hole circle
		(at 25.4 16.195)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "93f68e1d-e0c8-4acd-8aee-7ee84c2252f2")
	)
	(pad "23" thru_hole circle
		(at 25.4 13.655)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "982d0434-ac61-4490-b1fb-522f125b632b")
	)
	(pad "24" thru_hole circle
		(at 25.4 11.115)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "12d17e84-a342-4174-88ac-e2a7acacee54")
	)
	(pad "25" thru_hole circle
		(at 25.4 8.575)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "778ce7d9-f2a8-48ca-8cc7-7e9ba72394b4")
	)
	(pad "26" thru_hole circle
		(at 25.4 6.035)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "b141a7cd-0e87-4696-8ddd-7407e692711e")
	)
	(pad "27" thru_hole circle
		(at 25.4 3.495)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "544f9787-63ba-47bd-a260-4c44e7b66b09")
	)
	(pad "28" thru_hole circle
		(at 25.4 0.955)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "5845186c-3415-4149-957e-a6d6e46b2e3c")
	)
	(pad "29" thru_hole circle
		(at 25.4 -1.585)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "37d4792a-c87c-4267-9b5f-5dc82be6f57f")
	)
	(pad "30" thru_hole circle
		(at 25.4 -4.125)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(uuid "5c435429-3516-434f-bbbe-ca389802e99a")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-C3-DevKitM-1.stpZ"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
